FAQ content
How much torque does the Whyte Karve Evo RSX produce?
The Avinox M2S drive unit delivers up to 150Nm of maximum torque, with peak power of 1,300W and nominal power of 250W.
How much suspension travel does it have?
The Karve Evo RSX has 180mm of front travel from its RockShox ZEB Ultimate fork and 180mm of rear-wheel travel controlled by a custom-tuned RockShox Vivid Ultimate RC2T shock.
What battery does the Karve Evo RSX use?
It uses an 800Wh Avinox battery integrated into the frame. The battery can be removed for maintenance after removal of the motor.
How quickly does the battery charge?
With the included 12A fast charger, Whyte quotes approximately 1 hour 45 minutes from empty to 80%, and around 2 hours 23 minutes from empty to 100%. Actual charging time can vary with conditions.
Is it a mullet or full-29er bike?
It is supplied with a 29-inch front wheel and 27.5-inch rear wheel. It can be converted to a full-29er setup using Whyte’s compatible 29er Shape.It link and a suitable category 4-rated 29-inch rear wheel.
Can the geometry be adjusted?
Yes. The Shape.It Link V2 provides high and low settings, changing the head angle by 0.6 degrees and bottom-bracket height by 8mm.
What sizes are available?
Whyte lists Medium, Large and Extra Large. Contact The Endurance Hub for personal sizing advice before ordering.
How much does it weigh?
Whyte quotes 24.4kg for a size Large. Production-bike weight may vary slightly with size, setup and component tolerances.
Does it connect to an app?
Yes. The DPC100 display connects to the Avinox Ride app, giving access to ride information, system status and customisation options.
What warranty is included?
The bike is covered by Whyte’s applicable manufacturer warranty. Extended frame and pivot-bearing cover may require registration and is subject to Whyte’s current eligibility criteria, exclusions and terms. Ask The Endurance Hub for the latest details.

